## 

Look for traffic at each signal

Read from sensor

**Start**

if traffic at all signals

If traffic at 2 signals

If there is no traffic

Stop at current signal and wait for the traffic at other signal

Skip the other two 2 signals

Run normally